# m32r testcase for ldh $dr,@$sr
# mach(): m32r m32rx

	.include "testutils.inc"

	start

	.global ldh
ldh:
	mvaddr_h_gr r4, data_loc
	mvi_h_gr    r5, 0

	ldh r5, @r4

	test_h_gr r5, 0x1234 ; big endian processor

	pass

data_loc:
	.word 0x12345678

	pass
