# m32r testcase for addv3 $dr,$sr,#$simm16
# mach(): m32r m32rx

	.include "testutils.inc"

	start

	.global addv3
addv3:
	mvi_h_condbit 0
	mvi_h_gr r4, 1
	mvi_h_gr r5, 1

	addv3 r4, r5, #2

	bc not_ok

	test_h_gr r4, 3

	mvi_h_gr r5, 0x7fff8001

	addv3 r4, r5, #0x7fff

	bnc not_ok

	pass
not_ok:
	fail
