# m32r testcase for bc $disp8
# mach(): m32r m32rx

	.include "testutils.inc"

	start

	.global bc8
bc8:

	mvi_h_condbit 0
	bc.s test0fail
	bra test0pass
test0fail:
	fail
test0pass:

	mvi_h_condbit 1
	bc.s test1pass
	fail
test1pass:

	pass
