# m32r testcase for ldb $dr,@$sr
# mach(): m32r m32rx

	.include "testutils.inc"

	start

	.global ldb
ldb:
	mvaddr_h_gr r4, data_loc
	mvi_h_gr    r5, 0

	ldb r5, @r4

	test_h_gr r5, 0x12 ; big endian processor

	pass

data_loc:
	.word 0x12345678

