OUTPUT_FORMAT("coff-arm-little", "coff-arm-big", "coff-arm-little")
 SEARCH_DIR(/toolbin/xscale-coff/lib);
ENTRY(_start)
SECTIONS
{
  /* We start at 0x8000 because gdb assumes it (see FRAME_CHAIN).
     This is an artifact of the ARM Demon monitor using the bottom 32k
     as workspace (shared with the FP instruction emulator if
     present): */
  .text  0x8000 : {
    *(.init)
    *(.text)
    *(.glue_7t)
    *(.glue_7)
    *(.rdata)
     ___CTOR_LIST__ = .; __CTOR_LIST__ = . ; 
			LONG (-1); *(.ctors); *(.ctor); LONG (0); 
     ___DTOR_LIST__ = .; __DTOR_LIST__ = . ; 
			LONG (-1); *(.dtors); *(.dtor);  LONG (0); 
    *(.fini)
     etext  =  .;
     _etext  =  .;
  }
  .data 0x40000 + (. & 0xfffc0fff) : {
      __data_start__ = . ;
    *(.data)
     __data_end__ = . ;
     edata  =  .;
     _edata  =  .;
  }
  .bss  SIZEOF(.data) + ADDR(.data) :
  { 					
     __bss_start__ = . ;
    *(.bss)
    *(COMMON)
     __bss_end__ = . ;
  }
   end = .;
   _end = .;
   __end__ = .;
  .stab  0 (NOLOAD) : 
  {
    [ .stab ]
  }
  .stabstr  0 (NOLOAD) :
  {
    [ .stabstr ]
  }
}
